Brain Vision Data Exchange Header File Version 1.0
; Data created by the Vision Recorder

[Common Infos]
Codepage=UTF-8
DataFile=testVP02_St180.eeg
MarkerFile=testVP02_St180.vmrk
DataFormat=BINARY
; Data orientation: MULTIPLEXED=ch1,pt1, ch2,pt1 ...
DataOrientation=MULTIPLEXED
NumberOfChannels=64
; Sampling interval in microseconds
SamplingInterval=2000

[Binary Infos]
BinaryFormat=INT_16

[Channel Infos]
; Each entry: Ch<Channel number>=<Name>,<Reference channel name>,
; <Resolution in "Unit">,<Unit>, Future extensions..
; Fields are delimited by commas, some fields might be omitted (empty).
; Commas in channel names are coded as "\1".
Ch1=Fp1,,0.1,µV
Ch2=Fp2,,0.1,µV
Ch3=F7,,0.1,µV
Ch4=F3,,0.1,µV
Ch5=Fz,,0.1,µV
Ch6=F4,,0.1,µV
Ch7=F8,,0.1,µV
Ch8=FC5,,0.1,µV
Ch9=FC1,,0.1,µV
Ch10=FC2,,0.1,µV
Ch11=FC6,,0.1,µV
Ch12=T7,,0.1,µV
Ch13=C3,,0.1,µV
Ch14=Cz,,0.1,µV
Ch15=C4,,0.1,µV
Ch16=T8,,0.1,µV
Ch17=TP9,,0.1,µV
Ch18=CP5,,0.1,µV
Ch19=CP1,,0.1,µV
Ch20=CP2,,0.1,µV
Ch21=CP6,,0.1,µV
Ch22=TP10,,0.1,µV
Ch23=P7,,0.1,µV
Ch24=P3,,0.1,µV
Ch25=Pz,,0.1,µV
Ch26=P4,,0.1,µV
Ch27=P8,,0.1,µV
Ch28=PO9,,0.1,µV
Ch29=O1,,0.1,µV
Ch30=Oz,,0.1,µV
Ch31=O2,,0.1,µV
Ch32=PO10,,0.1,µV
Ch33=AF7,,0.1,µV
Ch34=AF3,,0.1,µV
Ch35=AF4,,0.1,µV
Ch36=AF8,,0.1,µV
Ch37=F5,,0.1,µV
Ch38=F1,,0.1,µV
Ch39=F2,,0.1,µV
Ch40=F6,,0.1,µV
Ch41=FT9,,0.1,µV
Ch42=FT7,,0.1,µV
Ch43=FC3,,0.1,µV
Ch44=FC4,,0.1,µV
Ch45=FT8,,0.1,µV
Ch46=FT10,,0.1,µV
Ch47=C5,,0.1,µV
Ch48=C1,,0.1,µV
Ch49=C2,,0.1,µV
Ch50=C6,,0.1,µV
Ch51=TP7,,0.1,µV
Ch52=CP3,,0.1,µV
Ch53=CPz,,0.1,µV
Ch54=CP4,,0.1,µV
Ch55=TP8,,0.1,µV
Ch56=P5,,0.1,µV
Ch57=P1,,0.1,µV
Ch58=P2,,0.1,µV
Ch59=P6,,0.1,µV
Ch60=PO7,,0.1,µV
Ch61=PO3,,0.1,µV
Ch62=POz,,0.1,µV
Ch63=PO4,,0.1,µV
Ch64=PO8,,0.1,µV

[Comment]

A m p l i f i e r  S e t u p
============================
Number of channels: 64
Sampling Rate [Hz]: 500
Sampling Interval [µS]: 2000

Channels
--------
#     Name      Phys. Chn.    Resolution / Unit   Low Cutoff [s]   High Cutoff [Hz]   Notch [Hz]    Series Res. [kOhm] Gradient         Offset
1     Fp1         1                0.1 µV             10              250              Off                0                 
2     Fp2         2                0.1 µV             10              250              Off                0                 
3     F7          3                0.1 µV             10              250              Off                0                 
4     F3          4                0.1 µV             10              250              Off                0                 
5     Fz          5                0.1 µV             10              250              Off                0                 
6     F4          6                0.1 µV             10              250              Off                0                 
7     F8          7                0.1 µV             10              250              Off                0                 
8     FC5         8                0.1 µV             10              250              Off                0                 
9     FC1         9                0.1 µV             10              250              Off                0                 
10    FC2         10               0.1 µV             10              250              Off                0                 
11    FC6         11               0.1 µV             10              250              Off                0                 
12    T7          12               0.1 µV             10              250              Off                0                 
13    C3          13               0.1 µV             10              250              Off                0                 
14    Cz          14               0.1 µV             10              250              Off                0                 
15    C4          15               0.1 µV             10              250              Off                0                 
16    T8          16               0.1 µV             10              250              Off                0                 
17    TP9         17               0.1 µV             10              250              Off                0                 
18    CP5         18               0.1 µV             10              250              Off                0                 
19    CP1         19               0.1 µV             10              250              Off                0                 
20    CP2         20               0.1 µV             10              250              Off                0                 
21    CP6         21               0.1 µV             10              250              Off                0                 
22    TP10        22               0.1 µV             10              250              Off                0                 
23    P7          23               0.1 µV             10              250              Off                0                 
24    P3          24               0.1 µV             10              250              Off                0                 
25    Pz          25               0.1 µV             10              250              Off                0                 
26    P4          26               0.1 µV             10              250              Off                0                 
27    P8          27               0.1 µV             10              250              Off                0                 
28    PO9         28               0.1 µV             10              250              Off                0                 
29    O1          29               0.1 µV             10              250              Off                0                 
30    Oz          30               0.1 µV             10              250              Off                0                 
31    O2          31               0.1 µV             10              250              Off                0                 
32    PO10        32               0.1 µV             10              250              Off                0                 
33    AF7         33               0.1 µV             10              250              Off                0                 
34    AF3         34               0.1 µV             10              250              Off                0                 
35    AF4         35               0.1 µV             10              250              Off                0                 
36    AF8         36               0.1 µV             10              250              Off                0                 
37    F5          37               0.1 µV             10              250              Off                0                 
38    F1          38               0.1 µV             10              250              Off                0                 
39    F2          39               0.1 µV             10              250              Off                0                 
40    F6          40               0.1 µV             10              250              Off                0                 
41    FT9         41               0.1 µV             10              250              Off                0                 
42    FT7         42               0.1 µV             10              250              Off                0                 
43    FC3         43               0.1 µV             10              250              Off                0                 
44    FC4         44               0.1 µV             10              250              Off                0                 
45    FT8         45               0.1 µV             10              250              Off                0                 
46    FT10        46               0.1 µV             10              250              Off                0                 
47    C5          47               0.1 µV             10              250              Off                0                 
48    C1          48               0.1 µV             10              250              Off                0                 
49    C2          49               0.1 µV             10              250              Off                0                 
50    C6          50               0.1 µV             10              250              Off                0                 
51    TP7         51               0.1 µV             10              250              Off                0                 
52    CP3         52               0.1 µV             10              250              Off                0                 
53    CPz         53               0.1 µV             10              250              Off                0                 
54    CP4         54               0.1 µV             10              250              Off                0                 
55    TP8         55               0.1 µV             10              250              Off                0                 
56    P5          56               0.1 µV             10              250              Off                0                 
57    P1          57               0.1 µV             10              250              Off                0                 
58    P2          58               0.1 µV             10              250              Off                0                 
59    P6          59               0.1 µV             10              250              Off                0                 
60    PO7         60               0.1 µV             10              250              Off                0                 
61    PO3         61               0.1 µV             10              250              Off                0                 
62    POz         62               0.1 µV             10              250              Off                0                 
63    PO4         63               0.1 µV             10              250              Off                0                 
64    PO8         64               0.1 µV             10              250              Off                0                 

S o f t w a r e  F i l t e r s
==============================
Disabled


Data Electrodes Selected Impedance Measurement Range: 0 - 100 kOhm
Ground Electrode Selected Impedance Measurement Range: 0 - 10 kOhm
Reference Electrode Selected Impedance Measurement Range: 0 - 10 kOhm
Impedance [kOhm] at 14:10:48 :
Fp1:         76
Fp2:         75
F7:          75
F3:          75
Fz:          76
F4:          75
F8:          75
FC5:         75
FC1:         76
FC2:         76
FC6:         75
T7:          76
C3:          76
Cz:          76
C4:          76
T8:          76
TP9:         75
CP5:         76
CP1:         76
CP2:         76
CP6:         76
TP10:        76
P7:          76
P3:          76
Pz:          76
P4:          76
P8:          76
PO9:         76
O1:          76
Oz:          76
O2:          76
PO10:        76
AF7:      Out of Range!
AF3:      Out of Range!
AF4:      Out of Range!
AF8:      Out of Range!
F5:       Out of Range!
F1:       Out of Range!
F2:       Out of Range!
F6:       Out of Range!
FT9:      Out of Range!
FT7:      Out of Range!
FC3:      Out of Range!
FC4:      Out of Range!
FT8:      Out of Range!
FT10:     Out of Range!
C5:       Out of Range!
C1:       Out of Range!
C2:       Out of Range!
C6:       Out of Range!
TP7:      Out of Range!
CP3:      Out of Range!
CPz:      Out of Range!
CP4:      Out of Range!
TP8:      Out of Range!
P5:       Out of Range!
P1:       Out of Range!
P2:       Out of Range!
P6:       Out of Range!
PO7:      Out of Range!
PO3:      Out of Range!
POz:      Out of Range!
PO4:      Out of Range!
PO8:      Out of Range!
Ref:         69
Gnd:      Out of Range!
