------------------------------------------
Setting up environment variables
---
LD_LIBRARY_PATH is .:/opt/matlab/R2016b/runtime/glnxa64:/opt/matlab/R2016b/bin/glnxa64:/opt/matlab/R2016b/sys/os/glnxa64:/opt/matlab/R2016b/sys/opengl/lib/glnxa64
processing sub-021
Warning: sampleinfo in the configuration is inconsistent with the actual data
 In '/mnt/beegfs/home/kosciessa/.mcrCache9.1/a3_ica0/mnt/beegfs/home/kosciessa/EEGManyPipelines/eegmp_preproc/tools/fieldtrip/utilities/private/fixsampleinfo.m' at line 100
 In '/mnt/beegfs/home/kosciessa/.mcrCache9.1/a3_ica0/mnt/beegfs/home/kosciessa/EEGManyPipelines/eegmp_preproc/tools/fieldtrip/utilities/ft_datatype_raw.m' at line 148
 In '/mnt/beegfs/home/kosciessa/.mcrCache9.1/a3_ica0/mnt/beegfs/home/kosciessa/EEGManyPipelines/eegmp_preproc/tools/fieldtrip/utilities/ft_checkdata.m' at line 277
 In '/mnt/beegfs/home/kosciessa/.mcrCache9.1/a3_ica0/mnt/beegfs/home/kosciessa/EEGManyPipelines/eegmp_preproc/tools/fieldtrip/ft_preprocessing.m' at line 288

Warning: reconstructing sampleinfo by assuming that the trials are consecutive segments of a continuous recording
the call to "ft_selectdata" took 1 seconds and required the additional allocation of an estimated 280 MB
preprocessing
preprocessing trial 1 from 1
the call to "ft_preprocessing" took 2 seconds and required the additional allocation of an estimated 296 MB
the input is raw data with 71 channels and 1933 trials
the call to "ft_selectdata" took 0 seconds and required the additional allocation of an estimated 1 MB
scaling data with 1 over 288.105469
concatenating data
concatenating trials...
Concatenating trial 620 from 1933Concatenating trial 1229 from 1933Concatenating trial 1846 from 1933Concatenating trial 1933 from 1933
concatenated data matrix size 71x966500
starting decomposition using runica

Input data size [71,966500] = 71 channels, 966500 frames
Finding 71 ICA components using extended ICA.
Kurtosis will be calculated initially every 1 blocks using 6000 data points.
Decomposing 191 frames per ICA weight ((5041)^2 = 966500 weights, Initial learning rate will be 0.001, block size 69.
Learning rate will be multiplied by 0.98 whenever angledelta >= 60 deg.
More than 32 channels: default stopping weight change 1E-7
Training will end when wchange < 1e-07 or after 512 steps.
Online bias adjustment will be used.
Removing mean of each channel ...
Final training data range: -1.39907 to 1.84829
Computing the sphering matrix...
Starting weights are the identity matrix ...
Sphering the data ...
Beginning ICA training ... first training step may be slow ...
Lowering learning rate to 0.0009 and starting again.
Lowering learning rate to 0.00081 and starting again.
Lowering learning rate to 0.000729 and starting again.
Lowering learning rate to 0.0006561 and starting again.
Lowering learning rate to 0.00059049 and starting again.
Lowering learning rate to 0.000531441 and starting again.
Lowering learning rate to 0.000478297 and starting again.
Lowering learning rate to 0.000430467 and starting again.
Lowering learning rate to 0.00038742 and starting again.
Lowering learning rate to 0.000348678 and starting again.
Lowering learning rate to 0.000313811 and starting again.
Lowering learning rate to 0.00028243 and starting again.
Lowering learning rate to 0.000254187 and starting again.
Lowering learning rate to 0.000228768 and starting again.
Lowering learning rate to 0.000205891 and starting again.
Lowering learning rate to 0.000185302 and starting again.
Lowering learning rate to 0.000166772 and starting again.
Lowering learning rate to 0.000150095 and starting again.
Lowering learning rate to 0.000135085 and starting again.
Lowering learning rate to 0.000121577 and starting again.
Lowering learning rate to 0.000109419 and starting again.
Lowering learning rate to 9.84771e-05 and starting again.
Lowering learning rate to 8.86294e-05 and starting again.
Lowering learning rate to 7.97664e-05 and starting again.
step 1 - lrate 0.000080, wchange 31.10090402, angledelta  0.0 deg
step 2 - lrate 0.000080, wchange 0.58361264, angledelta  0.0 deg
Lowering learning rate to 7.17898e-05 and starting again.
step 1 - lrate 0.000072, wchange 31.08606936, angledelta  0.0 deg
Lowering learning rate to 6.46108e-05 and starting again.
step 1 - lrate 0.000065, wchange 30.81810766, angledelta  0.0 deg
step 2 - lrate 0.000065, wchange 0.67348448, angledelta  0.0 deg
step 3 - lrate 0.000065, wchange 0.83225267, angledelta 84.9 deg
step 4 - lrate 0.000063, wchange 0.14040723, angledelta 80.4 deg
step 5 - lrate 0.000062, wchange 0.09746190, angledelta 72.7 deg
step 6 - lrate 0.000061, wchange 0.38495617, angledelta 107.4 deg
step 7 - lrate 0.000060, wchange 1.06824582, angledelta 150.2 deg
step 8 - lrate 0.000058, wchange 0.08063515, angledelta 91.0 deg
Lowering learning rate to 5.15115e-05 and starting again.
step 1 - lrate 0.000052, wchange 31.87037140, angledelta  0.0 deg
step 2 - lrate 0.000052, wchange 0.48326176, angledelta  0.0 deg
step 3 - lrate 0.000052, wchange 0.22767667, angledelta 84.0 deg
step 4 - lrate 0.000050, wchange 0.13126184, angledelta 66.8 deg
step 5 - lrate 0.000049, wchange 0.59311378, angledelta 87.6 deg
step 6 - lrate 0.000048, wchange 0.53264794, angledelta 147.2 deg
step 7 - lrate 0.000048, wchange 0.67721333, angledelta 153.7 deg
step 8 - lrate 0.000047, wchange 0.04933128, angledelta 109.1 deg
step 9 - lrate 0.000046, wchange 0.56164892, angledelta 72.5 deg
step 10 - lrate 0.000045, wchange 0.60393309, angledelta 158.8 deg
step 11 - lrate 0.000044, wchange 0.59378939, angledelta 163.3 deg
step 12 - lrate 0.000043, wchange 0.17203341, angledelta 154.6 deg
step 13 - lrate 0.000042, wchange 0.13735633, angledelta 43.3 deg
step 14 - lrate 0.000042, wchange 0.75617263, angledelta 151.6 deg
step 15 - lrate 0.000041, wchange 0.05555971, angledelta 140.7 deg
step 16 - lrate 0.000040, wchange 0.51634348, angledelta 46.7 deg
step 17 - lrate 0.000040, wchange 0.47014781, angledelta 135.7 deg
step 18 - lrate 0.000040, wchange 0.62561831, angledelta 166.1 deg
step 19 - lrate 0.000039, wchange 0.02859896, angledelta 112.9 deg
step 20 - lrate 0.000038, wchange 0.02506138, angledelta 102.0 deg
step 21 - lrate 0.000037, wchange 0.02086864, angledelta 110.9 deg
step 22 - lrate 0.000037, wchange 0.35528737, angledelta 89.8 deg
step 23 - lrate 0.000036, wchange 0.25320678, angledelta 26.7 deg
step 24 - lrate 0.000036, wchange 0.14107614, angledelta 152.7 deg
step 25 - lrate 0.000035, wchange 0.28781011, angledelta 34.2 deg
step 26 - lrate 0.000035, wchange 0.28957293, angledelta 152.3 deg
step 27 - lrate 0.000034, wchange 0.02846697, angledelta 128.8 deg
step 28 - lrate 0.000034, wchange 0.03355153, angledelta 133.2 deg
step 29 - lrate 0.000033, wchange 0.68111216, angledelta 136.1 deg
step 30 - lrate 0.000032, wchange 0.74670251, angledelta 171.1 deg
step 31 - lrate 0.000032, wchange 0.86072873, angledelta 169.1 deg
step 32 - lrate 0.000031, wchange 0.02971996, angledelta 90.8 deg
step 33 - lrate 0.000030, wchange 0.08463360, angledelta 106.6 deg
step 34 - lrate 0.000030, wchange 0.01671341, angledelta 115.6 deg
step 35 - lrate 0.000029, wchange 0.58709236, angledelta 107.3 deg
step 36 - lrate 0.000029, wchange 0.01698955, angledelta 116.3 deg
step 37 - lrate 0.000028, wchange 0.13584376, angledelta 119.4 deg
step 38 - lrate 0.000028, wchange 1.06925411, angledelta 163.6 deg
step 39 - lrate 0.000027, wchange 0.02152808, angledelta 55.9 deg
step 40 - lrate 0.000027, wchange 0.70586246, angledelta 169.5 deg
step 41 - lrate 0.000026, wchange 0.05829115, angledelta 153.7 deg
step 42 - lrate 0.000026, wchange 0.03492527, angledelta 147.6 deg
step 43 - lrate 0.000025, wchange 0.81878240, angledelta 144.5 deg
step 44 - lrate 0.000025, wchange 0.01647944, angledelta 123.5 deg
step 45 - lrate 0.000024, wchange 0.01259823, angledelta 106.0 deg
step 46 - lrate 0.000024, wchange 0.02814124, angledelta 119.3 deg
step 47 - lrate 0.000023, wchange 0.01574773, angledelta 79.0 deg
step 48 - lrate 0.000023, wchange 0.01896907, angledelta 131.0 deg
step 49 - lrate 0.000022, wchange 0.04322887, angledelta 67.6 deg
step 50 - lrate 0.000022, wchange 0.02514800, angledelta 146.2 deg
step 51 - lrate 0.000022, wchange 0.02173144, angledelta 140.4 deg
step 52 - lrate 0.000021, wchange 0.01554214, angledelta 132.7 deg
step 53 - lrate 0.000021, wchange 0.10768317, angledelta 66.4 deg
step 54 - lrate 0.000020, wchange 0.06728606, angledelta 159.3 deg
step 55 - lrate 0.000020, wchange 0.01304005, angledelta 70.0 deg
step 56 - lrate 0.000020, wchange 0.01045785, angledelta 102.2 deg
step 57 - lrate 0.000019, wchange 0.01689864, angledelta 124.9 deg
step 58 - lrate 0.000019, wchange 0.01542236, angledelta 137.4 deg
step 59 - lrate 0.000018, wchange 0.00982273, angledelta 122.6 deg
step 60 - lrate 0.000018, wchange 0.01852720, angledelta 96.4 deg
step 61 - lrate 0.000018, wchange 0.03070737, angledelta 141.7 deg
step 62 - lrate 0.000017, wchange 0.00788057, angledelta 99.4 deg
step 63 - lrate 0.000017, wchange 0.01665118, angledelta 114.1 deg
step 64 - lrate 0.000017, wchange 0.01871464, angledelta 142.7 deg
step 65 - lrate 0.000016, wchange 0.00770540, angledelta 119.9 deg
step 66 - lrate 0.000016, wchange 0.00958863, angledelta 105.7 deg
step 67 - lrate 0.000016, wchange 0.00683943, angledelta 118.7 deg
step 68 - lrate 0.000015, wchange 0.00729316, angledelta 114.9 deg
step 69 - lrate 0.000015, wchange 0.02496963, angledelta 116.9 deg
step 70 - lrate 0.000015, wchange 0.00719117, angledelta 99.6 deg
step 71 - lrate 0.000014, wchange 0.03650300, angledelta 108.4 deg
step 72 - lrate 0.000014, wchange 0.03188778, angledelta 154.7 deg
step 73 - lrate 0.000014, wchange 0.00775000, angledelta 123.8 deg
step 74 - lrate 0.000014, wchange 0.00664317, angledelta 123.0 deg
step 75 - lrate 0.000013, wchange 0.01605827, angledelta 119.2 deg
step 76 - lrate 0.000013, wchange 0.01886174, angledelta 146.0 deg
step 77 - lrate 0.000013, wchange 0.01136636, angledelta 141.8 deg
step 78 - lrate 0.000013, wchange 0.00969760, angledelta 78.6 deg
step 79 - lrate 0.000012, wchange 0.00673117, angledelta 128.7 deg
step 80 - lrate 0.000012, wchange 0.01522939, angledelta 85.9 deg
step 81 - lrate 0.000012, wchange 0.00573856, angledelta 97.5 deg
step 82 - lrate 0.000012, wchange 0.03246083, angledelta 112.3 deg
step 83 - lrate 0.000011, wchange 0.00528407, angledelta 109.6 deg
step 84 - lrate 0.000011, wchange 0.00511835, angledelta 120.7 deg
step 85 - lrate 0.000011, wchange 0.02502077, angledelta 98.2 deg
step 86 - lrate 0.000011, wchange 0.02578008, angledelta 155.1 deg
step 87 - lrate 0.000010, wchange 0.00501214, angledelta 116.8 deg
step 88 - lrate 0.000010, wchange 0.00461529, angledelta 119.9 deg
step 89 - lrate 0.000010, wchange 0.00472431, angledelta 122.9 deg
step 90 - lrate 0.000010, wchange 0.00490498, angledelta 112.3 deg
step 91 - lrate 0.000010, wchange 0.00422118, angledelta 124.5 deg
step 92 - lrate 0.000009, wchange 0.03077972, angledelta 112.1 deg
step 93 - lrate 0.000009, wchange 0.02088807, angledelta 157.1 deg
step 94 - lrate 0.000009, wchange 0.00442768, angledelta 80.7 deg
step 95 - lrate 0.000009, wchange 0.00402699, angledelta 113.5 deg
step 96 - lrate 0.000009, wchange 0.00603186, angledelta 119.6 deg
step 97 - lrate 0.000009, wchange 0.00608907, angledelta 85.1 deg
step 98 - lrate 0.000008, wchange 0.00516581, angledelta 131.1 deg
step 99 - lrate 0.000008, wchange 0.00439008, angledelta 96.6 deg
step 100 - lrate 0.000008, wchange 0.00509571, angledelta 96.6 deg
step 101 - lrate 0.000008, wchange 0.01279806, angledelta 133.8 deg
step 102 - lrate 0.000008, wchange 0.00570876, angledelta 138.6 deg
step 103 - lrate 0.000008, wchange 0.00312142, angledelta 117.8 deg
step 104 - lrate 0.000007, wchange 0.01776443, angledelta 93.6 deg
step 105 - lrate 0.000007, wchange 0.01377184, angledelta 154.6 deg
step 106 - lrate 0.000007, wchange 0.00462394, angledelta 69.5 deg
step 107 - lrate 0.000007, wchange 0.00448893, angledelta 133.0 deg
step 108 - lrate 0.000007, wchange 0.00254826, angledelta 112.9 deg
step 109 - lrate 0.000007, wchange 0.00280376, angledelta 119.4 deg
step 110 - lrate 0.000007, wchange 0.00497604, angledelta 116.9 deg
step 111 - lrate 0.000006, wchange 0.00278285, angledelta 113.8 deg
step 112 - lrate 0.000006, wchange 0.00400466, angledelta 110.4 deg
step 113 - lrate 0.000006, wchange 0.00371250, angledelta 130.7 deg
step 114 - lrate 0.000006, wchange 0.00301589, angledelta 128.6 deg
step 115 - lrate 0.000006, wchange 0.00409270, angledelta 93.5 deg
step 116 - lrate 0.000006, wchange 0.00219989, angledelta 108.0 deg
step 117 - lrate 0.000006, wchange 0.00338098, angledelta 111.3 deg
step 118 - lrate 0.000006, wchange 0.00243281, angledelta 125.3 deg
step 119 - lrate 0.000005, wchange 0.00547201, angledelta 93.4 deg
step 120 - lrate 0.000005, wchange 0.00255880, angledelta 127.2 deg
step 121 - lrate 0.000005, wchange 0.00386065, angledelta 92.7 deg
step 122 - lrate 0.000005, wchange 0.00213034, angledelta 98.1 deg
step 123 - lrate 0.000005, wchange 0.01155813, angledelta 116.7 deg
step 124 - lrate 0.000005, wchange 0.00279669, angledelta 135.0 deg
step 125 - lrate 0.000005, wchange 0.00419452, angledelta 80.4 deg
step 126 - lrate 0.000005, wchange 0.00274974, angledelta 135.6 deg
step 127 - lrate 0.000005, wchange 0.00180586, angledelta 106.1 deg
step 128 - lrate 0.000005, wchange 0.00415840, angledelta 103.9 deg
step 129 - lrate 0.000004, wchange 0.00171371, angledelta 104.7 deg
step 130 - lrate 0.000004, wchange 0.00496005, angledelta 103.3 deg
step 131 - lrate 0.000004, wchange 0.00925029, angledelta 149.5 deg
step 132 - lrate 0.000004, wchange 0.00157106, angledelta 100.1 deg
step 133 - lrate 0.000004, wchange 0.00349792, angledelta 105.9 deg
step 134 - lrate 0.000004, wchange 0.00287010, angledelta 73.4 deg
step 135 - lrate 0.000004, wchange 0.00737460, angledelta 141.4 deg
step 136 - lrate 0.000004, wchange 0.00533142, angledelta 152.1 deg
step 137 - lrate 0.000004, wchange 0.00763716, angledelta 152.5 deg
step 138 - lrate 0.000004, wchange 0.00221031, angledelta 137.5 deg
step 139 - lrate 0.000004, wchange 0.00124446, angledelta 117.6 deg
step 140 - lrate 0.000004, wchange 0.00173014, angledelta 120.9 deg
step 141 - lrate 0.000004, wchange 0.00508450, angledelta 132.5 deg
step 142 - lrate 0.000003, wchange 0.00155441, angledelta 132.0 deg
step 143 - lrate 0.000003, wchange 0.00502410, angledelta 73.6 deg
step 144 - lrate 0.000003, wchange 0.00740639, angledelta 155.1 deg
step 145 - lrate 0.000003, wchange 0.00351071, angledelta 151.0 deg
step 146 - lrate 0.000003, wchange 0.00142485, angledelta 81.0 deg
step 147 - lrate 0.000003, wchange 0.00207791, angledelta 130.7 deg
step 148 - lrate 0.000003, wchange 0.00106799, angledelta 105.8 deg
step 149 - lrate 0.000003, wchange 0.00248289, angledelta 102.5 deg
step 150 - lrate 0.000003, wchange 0.00476450, angledelta 146.4 deg
step 151 - lrate 0.000003, wchange 0.00192778, angledelta 58.5 deg
step 152 - lrate 0.000003, wchange 0.00409340, angledelta 142.9 deg
step 153 - lrate 0.000003, wchange 0.00107321, angledelta 78.8 deg
step 154 - lrate 0.000003, wchange 0.00137441, angledelta 128.1 deg
step 155 - lrate 0.000003, wchange 0.00085019, angledelta 115.1 deg
step 156 - lrate 0.000003, wchange 0.00153956, angledelta 115.1 deg
step 157 - lrate 0.000003, wchange 0.00127364, angledelta 135.3 deg
step 158 - lrate 0.000003, wchange 0.00087448, angledelta 102.0 deg
step 159 - lrate 0.000002, wchange 0.00077460, angledelta 125.1 deg
step 160 - lrate 0.000002, wchange 0.00081058, angledelta 122.4 deg
step 161 - lrate 0.000002, wchange 0.00069935, angledelta 116.8 deg
step 162 - lrate 0.000002, wchange 0.00073090, angledelta 117.2 deg
step 163 - lrate 0.000002, wchange 0.00114484, angledelta 125.8 deg
step 164 - lrate 0.000002, wchange 0.00082699, angledelta 88.5 deg
step 165 - lrate 0.000002, wchange 0.00256036, angledelta 131.2 deg
step 166 - lrate 0.000002, wchange 0.00072006, angledelta 129.5 deg
step 167 - lrate 0.000002, wchange 0.00099231, angledelta 128.5 deg
step 168 - lrate 0.000002, wchange 0.00243480, angledelta 141.2 deg
step 169 - lrate 0.000002, wchange 0.00050191, angledelta 114.4 deg
step 170 - lrate 0.000002, wchange 0.00642506, angledelta 85.5 deg
step 171 - lrate 0.000002, wchange 0.00982160, angledelta 165.4 deg
step 172 - lrate 0.000002, wchange 0.00095622, angledelta 140.6 deg
step 173 - lrate 0.000002, wchange 0.00048315, angledelta 95.3 deg
step 174 - lrate 0.000002, wchange 0.00049326, angledelta 123.9 deg
step 175 - lrate 0.000002, wchange 0.00039103, angledelta 118.3 deg
step 176 - lrate 0.000002, wchange 0.00050758, angledelta 112.1 deg
step 177 - lrate 0.000002, wchange 0.00040672, angledelta 110.5 deg
step 178 - lrate 0.000002, wchange 0.00045089, angledelta 120.8 deg
step 179 - lrate 0.000002, wchange 0.00072702, angledelta 88.9 deg
step 180 - lrate 0.000002, wchange 0.00033760, angledelta 114.1 deg
step 181 - lrate 0.000002, wchange 0.00064597, angledelta 106.7 deg
step 182 - lrate 0.000002, wchange 0.00031073, angledelta 106.9 deg
step 183 - lrate 0.000002, wchange 0.00067614, angledelta 112.0 deg
step 184 - lrate 0.000002, wchange 0.00164991, angledelta 143.4 deg
step 185 - lrate 0.000001, wchange 0.00028085, angledelta 105.1 deg
step 186 - lrate 0.000001, wchange 0.00085736, angledelta 101.5 deg
step 187 - lrate 0.000001, wchange 0.00090058, angledelta 147.7 deg
step 188 - lrate 0.000001, wchange 0.00198225, angledelta 151.5 deg
step 189 - lrate 0.000001, wchange 0.00026392, angledelta 119.3 deg
step 190 - lrate 0.000001, wchange 0.00027339, angledelta 123.9 deg
step 191 - lrate 0.000001, wchange 0.00084686, angledelta 126.4 deg
step 192 - lrate 0.000001, wchange 0.00042066, angledelta 61.5 deg
step 193 - lrate 0.000001, wchange 0.00035062, angledelta 137.7 deg
step 194 - lrate 0.000001, wchange 0.00103465, angledelta 137.3 deg
step 195 - lrate 0.000001, wchange 0.00084225, angledelta 153.8 deg
step 196 - lrate 0.000001, wchange 0.00016332, angledelta 92.9 deg
step 197 - lrate 0.000001, wchange 0.00016157, angledelta 117.9 deg
step 198 - lrate 0.000001, wchange 0.00034482, angledelta 120.4 deg
step 199 - lrate 0.000001, wchange 0.00038103, angledelta 142.3 deg
step 200 - lrate 0.000001, wchange 0.00012901, angledelta 104.4 deg
step 201 - lrate 0.000001, wchange 0.00021553, angledelta 111.2 deg
step 202 - lrate 0.000001, wchange 0.00020148, angledelta 132.0 deg
step 203 - lrate 0.000001, wchange 0.00010970, angledelta 108.1 deg
step 204 - lrate 0.000001, wchange 0.00017299, angledelta 106.4 deg
step 205 - lrate 0.000001, wchange 0.00024427, angledelta 135.4 deg
step 206 - lrate 0.000001, wchange 0.00036853, angledelta 59.6 deg
step 207 - lrate 0.000001, wchange 0.00029177, angledelta 130.3 deg
step 208 - lrate 0.000001, wchange 0.00010172, angledelta 119.5 deg
step 209 - lrate 0.000001, wchange 0.00024484, angledelta 90.8 deg
step 210 - lrate 0.000001, wchange 0.00024899, angledelta 142.3 deg
step 211 - lrate 0.000001, wchange 0.00008484, angledelta 86.4 deg
step 212 - lrate 0.000001, wchange 0.00015665, angledelta 90.4 deg
step 213 - lrate 0.000001, wchange 0.00013532, angledelta 136.5 deg
step 214 - lrate 0.000001, wchange 0.00009160, angledelta 128.7 deg
step 215 - lrate 0.000001, wchange 0.00007803, angledelta 124.2 deg
step 216 - lrate 0.000001, wchange 0.00005992, angledelta 116.4 deg
step 217 - lrate 0.000001, wchange 0.00008068, angledelta 115.4 deg
step 218 - lrate 0.000001, wchange 0.00007733, angledelta 127.1 deg
step 219 - lrate 0.000001, wchange 0.00010742, angledelta 131.3 deg
step 220 - lrate 0.000001, wchange 0.00015999, angledelta 139.0 deg
step 221 - lrate 0.000001, wchange 0.00023280, angledelta 147.8 deg
step 222 - lrate 0.000001, wchange 0.00007645, angledelta 138.6 deg
step 223 - lrate 0.000001, wchange 0.00003955, angledelta 117.5 deg
step 224 - lrate 0.000001, wchange 0.00006909, angledelta 92.5 deg
step 225 - lrate 0.000001, wchange 0.00009432, angledelta 137.0 deg
step 226 - lrate 0.000001, wchange 0.00006414, angledelta 136.3 deg
step 227 - lrate 0.000001, wchange 0.00002986, angledelta 112.9 deg
step 228 - lrate 0.000001, wchange 0.00004083, angledelta 100.5 deg
step 229 - lrate 0.000001, wchange 0.00013347, angledelta 130.5 deg
step 230 - lrate 0.000001, wchange 0.00007638, angledelta 147.5 deg
step 231 - lrate 0.000001, wchange 0.00006463, angledelta 56.0 deg
step 232 - lrate 0.000001, wchange 0.00002888, angledelta 117.8 deg
step 233 - lrate 0.000001, wchange 0.00002934, angledelta 119.7 deg
step 234 - lrate 0.000001, wchange 0.00003648, angledelta 122.4 deg
step 235 - lrate 0.000001, wchange 0.00002025, angledelta 114.9 deg
step 236 - lrate 0.000001, wchange 0.00003145, angledelta 95.6 deg
step 237 - lrate 0.000001, wchange 0.00006140, angledelta 135.2 deg
step 238 - lrate 0.000001, wchange 0.00003268, angledelta 136.3 deg
step 239 - lrate 0.000001, wchange 0.00001891, angledelta 82.0 deg
step 240 - lrate 0.000001, wchange 0.00001516, angledelta 115.3 deg
step 241 - lrate 0.000000, wchange 0.00001876, angledelta 103.7 deg
step 242 - lrate 0.000000, wchange 0.00001563, angledelta 89.4 deg
step 243 - lrate 0.000000, wchange 0.00001335, angledelta 95.3 deg
step 244 - lrate 0.000000, wchange 0.00002751, angledelta 116.9 deg
step 245 - lrate 0.000000, wchange 0.00001600, angledelta 127.4 deg
step 246 - lrate 0.000000, wchange 0.00001123, angledelta 118.2 deg
step 247 - lrate 0.000000, wchange 0.00003902, angledelta 76.9 deg
step 248 - lrate 0.000000, wchange 0.00002209, angledelta 140.4 deg
step 249 - lrate 0.000000, wchange 0.00000776, angledelta 93.1 deg
step 250 - lrate 0.000000, wchange 0.00001661, angledelta 92.7 deg
step 251 - lrate 0.000000, wchange 0.00000847, angledelta 81.7 deg
step 252 - lrate 0.000000, wchange 0.00002549, angledelta 76.6 deg
step 253 - lrate 0.000000, wchange 0.00001633, angledelta 142.5 deg
step 254 - lrate 0.000000, wchange 0.00000964, angledelta 67.5 deg
step 255 - lrate 0.000000, wchange 0.00000558, angledelta 114.0 deg
step 256 - lrate 0.000000, wchange 0.00000818, angledelta 112.8 deg
step 257 - lrate 0.000000, wchange 0.00000819, angledelta 76.7 deg
step 258 - lrate 0.000000, wchange 0.00000835, angledelta 129.8 deg
step 259 - lrate 0.000000, wchange 0.00000384, angledelta 102.4 deg
step 260 - lrate 0.000000, wchange 0.00001000, angledelta 96.9 deg
step 261 - lrate 0.000000, wchange 0.00000325, angledelta 95.9 deg
step 262 - lrate 0.000000, wchange 0.00000440, angledelta 104.7 deg
step 263 - lrate 0.000000, wchange 0.00000326, angledelta 93.4 deg
step 264 - lrate 0.000000, wchange 0.00000396, angledelta 90.6 deg
step 265 - lrate 0.000000, wchange 0.00000885, angledelta 129.2 deg
step 266 - lrate 0.000000, wchange 0.00000453, angledelta 136.0 deg
step 267 - lrate 0.000000, wchange 0.00000251, angledelta 91.7 deg
step 268 - lrate 0.000000, wchange 0.00000267, angledelta 98.7 deg
step 269 - lrate 0.000000, wchange 0.00000211, angledelta 104.3 deg
step 270 - lrate 0.000000, wchange 0.00000397, angledelta 95.6 deg
step 271 - lrate 0.000000, wchange 0.00000224, angledelta 75.1 deg
step 272 - lrate 0.000000, wchange 0.00000501, angledelta 124.4 deg
step 273 - lrate 0.000000, wchange 0.00000242, angledelta 129.1 deg
step 274 - lrate 0.000000, wchange 0.00000126, angledelta 94.0 deg
step 275 - lrate 0.000000, wchange 0.00000127, angledelta 104.9 deg
step 276 - lrate 0.000000, wchange 0.00000164, angledelta 106.4 deg
step 277 - lrate 0.000000, wchange 0.00000141, angledelta 115.6 deg
step 278 - lrate 0.000000, wchange 0.00000257, angledelta 75.7 deg
step 279 - lrate 0.000000, wchange 0.00000145, angledelta 127.4 deg
step 280 - lrate 0.000000, wchange 0.00000109, angledelta 115.4 deg
step 281 - lrate 0.000000, wchange 0.00000110, angledelta 115.5 deg
step 282 - lrate 0.000000, wchange 0.00000087, angledelta 107.4 deg
step 283 - lrate 0.000000, wchange 0.00000095, angledelta 108.1 deg
step 284 - lrate 0.000000, wchange 0.00000289, angledelta 68.2 deg
step 285 - lrate 0.000000, wchange 0.00000246, angledelta 142.8 deg
step 286 - lrate 0.000000, wchange 0.00000064, angledelta 120.3 deg
step 287 - lrate 0.000000, wchange 0.00000056, angledelta 92.6 deg
step 288 - lrate 0.000000, wchange 0.00000057, angledelta 96.6 deg
step 289 - lrate 0.000000, wchange 0.00000145, angledelta 117.2 deg
step 290 - lrate 0.000000, wchange 0.00000054, angledelta 122.8 deg
step 291 - lrate 0.000000, wchange 0.00000045, angledelta 85.4 deg
step 292 - lrate 0.000000, wchange 0.00000058, angledelta 113.5 deg
step 293 - lrate 0.000000, wchange 0.00000030, angledelta 99.5 deg
step 294 - lrate 0.000000, wchange 0.00000044, angledelta 99.5 deg
step 295 - lrate 0.000000, wchange 0.00000064, angledelta 69.4 deg
step 296 - lrate 0.000000, wchange 0.00000026, angledelta 97.1 deg
step 297 - lrate 0.000000, wchange 0.00000071, angledelta 96.9 deg
step 298 - lrate 0.000000, wchange 0.00000056, angledelta 48.7 deg
step 299 - lrate 0.000000, wchange 0.00000023, angledelta 82.5 deg
step 300 - lrate 0.000000, wchange 0.00000042, angledelta 87.2 deg
step 301 - lrate 0.000000, wchange 0.00000021, angledelta 112.4 deg
step 302 - lrate 0.000000, wchange 0.00000027, angledelta 109.1 deg
step 303 - lrate 0.000000, wchange 0.00000018, angledelta 86.8 deg
step 304 - lrate 0.000000, wchange 0.00000035, angledelta 80.6 deg
step 305 - lrate 0.000000, wchange 0.00000034, angledelta 130.7 deg
step 306 - lrate 0.000000, wchange 0.00000019, angledelta 119.1 deg
step 307 - lrate 0.000000, wchange 0.00000012, angledelta 100.7 deg
step 308 - lrate 0.000000, wchange 0.00000011, angledelta 97.3 deg
step 309 - lrate 0.000000, wchange 0.00000015, angledelta 85.5 deg
step 310 - lrate 0.000000, wchange 0.00000028, angledelta 118.2 deg
step 311 - lrate 0.000000, wchange 0.00000008, angledelta 95.6 deg
Sorting components in descending order of mean projected variance ...
the call to "ft_componentanalysis" took 3996 seconds and required the additional allocation of an estimated 1527 MB
